NOAA P-3 N43RF

NAME Flt #7

Flight ID: I040724

Sensor or system	Number or Name

INE	2

Accelerometer	2

Temperature Probe	1

Dew Point Probe	2 (EdgeTech)

Altitude (for vertical wind)	Pressure Altitude

Static Pressure	Rosemount Fuselage

Dynamic Pressure	Rosemount Fuselage

Time Source	Micro 99

Constants File	CO3042.CON

Notes:

There were no time/data gaps.

Dewpoint sensor #2 (DW2) was fixed during the following time periods: 1758Z - 1801Z and

181031Z - 181230Z. Also DW2 values were replaced with DW1 values during the following time frames: 135354Z - 135544Z, 143700Z - 143831Z, 144207Z - 144307Z, 145815Z - 145932Z, 152934Z - 153053Z, 160120Z - 160520Z, 165452Z - 170147Z, 170509Z - 170547Z, and 200934Z - 201901Z.

The King liquid water probe and the CO2 side radiometer were inoperative for the entire mission.

All other instruments worked optimally during the flight.

The aircraft INE positions were renavigated with respect to GPS.

SPECIAL NOTE!!!	Locations 80, 81 and 82 of record five on the standard tape contain

vertical ground, vertical air and vertical speeds, respectively, computed

using Dave Jorgensen's vertical wind algorithm.

It is recommended that these values be used for vertical wind analysis.

Takeoff	Landing

Aircraft Static Pressure	1010.9mb	1009.9	mb

Corrected Tower Pressure	1009.8mb	1008.8 mb

Flight Director:	A. Barry Damiano

Phone #:	(813) 828-3310 ext. 3073