Description of common area arrays for RAMS '84 software

Version 3.51 25 May 05 ASG Revised SFMR storage for new HRD filter

Version 3.5 11 May 04 ASG New Version of AOC SFMR data stream

Version 3.4 10 Feb 03 ASG Added stuff for AOC SFMR

Version 3.32 5 Sep 00 ASG Modify BR2G word assigns for actual instr output

Version 3.31 16 Aug 00 ASG Redefine HtSel

Version 3.3 19 Jun 00 ASG Added Epplys, Ashtech BR2G GPS, new serial

Version 3.2 5 Nov 99 ASG Support for Recording to Disk

Version 3.1 15 Sep 98 ASG AVAPS data in T5

Version 3.0 2 Apr 98 ASG Tape buffering in EMA, no fast tape disable

Version 2.9 6 Mar 96 ASG Interim version w/data passed in EMA

Version 2.8 7 Apr 94 ASG Replace Trimble with Collins Rcvr 3M GPS

Version 2.7 21 Sep 93 ASG New PQ/PS dynamic calc (mod. to CNS)

Version 2.6 11 Mar 92 ASG Replaced ONE with Trimble Nav

Version 2.5 17 Sep 91 ASG Added ASDL-VI stuff & rearranged IT1,T5,etc.

Version 2.4 20 Mar 91 ASG Revamped PQ,Flow Angle,TT,TW & all IT1 stuff

Version 2.3 11 Apr 90 ASG T3 in, Loran chan info out

ISEC - 220 integer array; contains 1 sec of raw slow data

ADC - 80 real array; ADC channel data - floated and converted to volts

T1 thru T3 are used to transfer and modify data values. T5 is the

final destination table. Each entry in T1 & T2 consists of 3 or 5

real words. The first word is equivalenced to 2 integers which

specify source and destination array addresses. T3 takes two sources

from T5 or ADC (indicies above T5_siz map to ADC), scales and offsets

them, performs the selected math (+,-,*,/) and stores the result in

T5. 1st two words are treated as 4 integers (source 1 addr, source 2

addr, operation, dest addr).

T1 - 3x50 real array; constants for moving data from ADC to T5

50*(Source/Dest,A,B) for Dest = A*X + B

T2 - 5x10 real array; 4 coef array for moving data from ADC to T5

10*(Source/Dest,A,B,C,D) for Dest = AX**3 + BX**2 + C*X + D

T3 - 6x20 real array; array for taking two source numbers (in T5 and/or

ADC), scaling each, doing a selected operation, store result.

20*(Source1/Source2,Operation/Dest,A1,B1,A2,B2)

for dest = (A1*S1 + B1) {+,-,*,/} (A2*S2 + B2)

DACTBL - 3x16 real array; array for DAC output data. First real word

is Source/Dest (Source is loc. in T5, Dest is DAC chan 0-15)

16*(source/dest,offset,scale) for dest = (source+offset)*scale

IT1 - 30 integer array; array of flags for global control and selection

CNS - 25 real array; general constants for met. calc.

NAME - 3x20 integer array; table of names for scheduling

each name is 3 integers - 6 characters

IAUCH- 40 integer array; device pointers for IAU channels

ISFLG- 30 integer array; flags for interprogram communication

ISERR- 20 integer array; error flags from vital programs

ISINFO- 19 integer array; Misc. system info - not filled by Rams_Common

IDERR- 20 integer array; met. data error flags

T5 - 250 real array; storage for computed met. data

ASDLDAT - 16 real array; averaged flight level data for ASDL

EYE - 2 real array; lat & long of eye position (for To/From display)

DEST - 2 real array; lat & long of destination position (")

EYENAME - 2 integer (4 char) array; name identifier for eye coord.

DESTNAME - 2 integer (4 char) array; name identifier for dest coord.

IPROJECT - 12 integer (24 char) array; project name

IAUSTAT - 40 integer array; storage for received IAU status burst

IAUSET - 20 integer (40 byte) array; storage for 1st config. byte

for each IAU channel; used to determine card & device type

ADCSTAT - 50 integer array; storage for received ADC status burst

*

**********************************************

* Detailed Description of Common Arrays *

**********************************************

*

* Array - ISEC

*

Array Filled

Loc. AKA by Description

1 Setup MS Byte - Slow tape ID, LS Byte - Acft #

2 Setup size of slow tape logical record == 220

3-8 Setup Micro 29 time - yr,mo,da,hr,mn,sc; updated by fast

9-11 Fast TBG 1 time - hr,min,sec; binary (not BCD)

12-14 Fast TBG 2 time -same as TBG 1

15-17 GPS_Time Fast 3M GPS Time of fix - hr,min,sec; same as TBG's

18-19 GPS_Dat Fast 3M GPS Altitude - MS bit = -102400*32 ft

20-21 Fast 3M GPS Latitude - MS bit = -PI*4 radians

22-23 Fast 3M GPS Longitude - MS bit = -PI*4 radians

24-25 Fast 3M GPS North Vel. - MS bit = -1638.4*2 knots

26-27 Fast 3M GPS East Vel. - MS bit = -1638.4*2 knots

28-29 Fast 3M GPS Vert. Vel. - MS bit = -2048*2 ft/sec

30 Fast BR2G GPS Data Time; 0 to 36000, lsb = 1/100 sec

31 Fast BR2G GPS Altitude; +/- 32767, lsb = 1 ft

32-33 Fast BR2G GPS Latitude; msb = -PI*4 radians

34-35 Fast BR2G GPS Longitude; msb = -PI*4 radians

36 Fast BR2G GPS Status and Horiz. Dilution of Precision

bits 15,14: 00 - no position, 01 - uncorrected,

10 - diff corrected, 11 - almanac used

bits 13-8: # of satellites used

ls byte - HDOP 00 to 99

37 Spare

38 Fast 3M GPS North Accel. - MS bit = -128 m/s**2

39 Fast 3M GPS East Accel. - MS bit = -128 m/s**s

40 Fast 3M GPS Vert. Accel. - MS bit = -128 m/s**2

41 Fast 3M GPS Chan 1 Status 1 \ See Rcvr 3M Spec. for

42 Fast 3M GPS Chan 1 Status 2 / bit assignments

43-50 Fast 3M GPS Chan 2-5 Status - same format as Chan 1

51 Fast 3M GPS Figure of Merit word - See Rcvr 3M spec.

Note: Time FOM from word 64 is in reserved bits

(12,11,5,4 in HP notation; 3,4,10,11 in 3M/DEC)

52 Fast 3M GPS expected horiz. error - LS bit = 1 meter

53 Fast 3M GPS expected vert. error - LS bit = 1 meter

54 Spare

55-56 Fast INE 1 Altitude - MS bit = -102400*32 ft

57-58 Fast INE 1 Latitude - MS bit = -PI*4 radians

59-60 Fast INE 1 Longitude - MS bit = -PI*4 radians

61-62 Fast INE 1 North Vel. - MS bit = -1638.4*2 knots

63-64 Fast INE 1 East Vel. - MS bit = -1638.4*2 knots

65-66 Fast INE 1 Vert. Speed - MS bit = -2048*2 ft/sec

67-68 Fast INE 1 Drift Angle - MS bit = -PI*4 radians

69-70 Fast INE 1 Heading - MS bit = -PI*4 radians

71-72 Fast INE 1 Pitch Angle - MS bit = -PI*4 radians

73-74 Fast INE 1 Roll Angle - MS bit = -PI*4 radians

75-94 Fast INE 2 Data - same as INE 1

95 Fast APN-232 RA Data in meters; 1 sec avg

96 Fast Spare; 1 sec avg

97 Fast Spare; 1 sec avg

98 Fast APN-159 RA synchro data in meters; 1 sec avg

99 Fast APN-159 RA parallel encoder data in meters

100 INEflg Fast # of INE bursts avg'd this sec; ms byte - INE #1

ls byte - INE #2

101 GPSflg Fast GPS & APN232 RA burst count;

bits 15-12: Ashtech BR2G GPS # of bursts

bits 11-8 : Collins 3M GPS # of bursts

bits 7-0 : APN232 RA # of words avg'd this sec

102 GarFlg Fast # of ISEC word 96 & 97 samples avg'd this sec;

ms byte - ISEC(96), ls byte - ISEC(97)

103 Dig_Err Fast Error flags for Dig. Avg.; bit 0 for APN232, etc.

104 spare

105 ADCstatus ASSRV ADC unit status - from ADC slow data burst

106 IAUstatus Fast IAU unit status - from IAU burst

107 OperSel Slow Operator selections: ms nybl - temp probe,

nybl 2 - nav. unit, nybl 3 - Alt. source

ls nybl - dewpoint unit

108 Fast status from Wing Wiring Junction Box

109 Fast status from Cloud Physics Station

110 Fast status from Flight Director Station

111 Fast spare

112 Fast event switch data - Nav,Sta1,Sta2,Sta3

113 Fast event switch data - Nrack,Sta5,C3X,Sta7

114 Fast event switch data - F/D,Pilot

115 Fast

116 Fast

117 Fast Formvar count

118 Fast Formvar speed

119 Fast Vaisala Cabin Pres in mBar*20; LSB is update flag

120-128 Fast Optional user serial data

129 Fast SFMR Slot A Antenna Value (Counts)

130 Fast " " " Warm Cal Load Value (Counts)

131 Fast " " " Hot Cal Load Value (Counts)

132 Fast " " " Cold Cal ( **future use )

133-136 Fast SFMR Slot B Values - same assignments as Slot A

137 Fast SFMR Thermistor and Housekeeping Data - see below

138 Fast SFMR Update Status word

Bit 0-2 - Slot A Freq | 000 - Nothing in Slot

3-5 - Slot B Freq | 001 - Freq #0 (4.74 GHz)

| 010 - Freq #1 (5.31 GHz)

| :

| 110 - Freq #5 (7.09 GHz)

6-8 - ISEC(137) data | 000 - Nothing in loc

| 001 - MS Byte - t0

| LS Byte - t1

| 010 - MS Byte - t2

| LS Byte - t3

| 011 - MS Byte - t4

| LS Byte - t5

| 100 - MS Byte - t6 **

| LS Byte - tr

| 101 - MS Byte - mode

| LS Byte - Status

| 110 - Internal Press

| (counts)

139 Fast M29 10 mSec tic when time was read - use for clock

drift tracking

140-219 ASSRV raw integer ADC data from slow burst

220 Slow checksum for this second

*

* Array - IT1

*

Array Modified

Loc. AKA by Description

1 TempSel Select Temp probe for Met. calc: 1-Temp#1, 2-Temp#2

2 NavSel Select Nav. for Met. calc: 1-INE1, 2-INE2,

0-GPS position w/INE #1 velocity and attitude

3-GPS position w/INE #2 velocity and attitude

3 AltSel Select Altitude source for Met. calc: 0-PA, 1-GA1,

2-GA2

4 DewSel Select Dewpoint source for met. calc: 1-Dewpt #1,

2-Dewpt #2, 3-Dewpt #3

5 PRate Print rate; 0-no print, >0 - rate in sec, <0 - ff

6 FlowSel Select flow angle sensors for AA & SA calc:

0-AP1,BP1 1-AP2,BP1 2-AP1,BP2 3-AP2,BP2

7 WZsel Select Vert. Accel. for WZ; 1-VA #1, 2-VA #2

8 PDsplOn Primary Fixed Format Display; 0-off,>0-on,<0-cls

9 SDsplOn Secondary Fixed Format Display; " " "

10 TDsplOn Tertiary Fixed Format Display; " " "

11 DiskEnab Disk Recording Enable; 0-no disk rec, 1-enabled

12 SecEnab Secondary Tape enable; 0-no sec tape, 1-sec tape on

13 PrmLu Primary Mag. Tape Logical Unit - maintained by Tape

a neg. Lu means tape recording is disabled

14 AsdlLu LU of RS-232 Port connected to ASDL-VI Computer

15 ReSync Set M29 time to TBG (1 - TBG#1; 2 - TBG#2) once

16 AsdFltr Length of ASDL RECCO data filter in seconds

17 AsdSlot Asdl Transmit slot selection: -1 - Default for this

acft; else one bit for each 5 min block, bit 0

selects :00 to :04, bit 1 selects :05 to :09, etc.

18 PSsel Select system PS; 1-3 for PS1-PS3

19 PQsel Select system PQ; 1-4 for PQ1-PQ4

20 RAflg RA & GA select: 0 - Do not use - (default to RA1)

1 - RA = RA1 (APN159 synchro)

2 - RA = RA2 (APN232)

3 - RA = RA3 (GPS MSL)

Selected RA is used to calc GA1. GA2 is from

RA3 (GPS). Positive RAflg selects GA1 for GA,

Negative RAflg selects GA2 for GA. For example,

-1 selects RA = RA1 and GA = GA2

21 AsdFreq Time between ASDL Flight Level data samples in Sec.

Pos. # only collects samples if GS>10m/s

Neg. # collects samples all the time.

22 AsdBlok Time between Flight Level block transmissions to

ASDL-VI in Minutes

23 UserPat1 | Word patterns for user serial data. Each UserPat

24 UserPat2 | is for one ASCII stream (see IAUCH for chan).

| Each bit keeps (=1) or discards (=0) an ASCII

| word within the user stream. LS bit is for

| 1st word, etc.

25 LanEnab Enable Lan Broadcast: 1 - BCast on, 0 - BCast off

26 SFMRSel Select SFMR device for ASDL output:

0 - First valid value, search order is next

1 - AOC SFMR

2 - UMass or Quadrant SFMR

27-30 Spare

*

* Array - CNS

*

*

Array

Loc. Description

1 AAM1 offset - converts attack pressure #1 to ang. of attack #1

2 AAM1 slope

3 SAM1 offset - converts sideslip pressure #1 to ang. of sideslip #1

4 SAM1 slope

5 AAM2 offset - same as CNS(1-4), but for nose flow angle sensors

6 AAM2 slope

7 SAM2 offset

8 SAM2 slope

9 PQWNG offset - PQ2M correction because it's on the wingtip

10 PSWNG offset - PS2M " " " " " "

11 PQER1 coefficient for PQERR equation

12 PQER2 coefficient " " "

13 PQER3 coefficient " " "

14 PQER4 coefficient " " "

15 PSerr offset - 1st term in PSerr calc

16 PSerr slope1 - multiplier for 2nd term in PSerr calc

17 PSerr scale1 - scale factor (divisor) for 2nd term in PSerr calc

18 PSerr power1 - exponent for 2nd term in PSerr calc

19 PSerr slope2 - multiplier for 3rd term; set = 0 if no 3rd term

20 PSerr scale2 - divisor for 3rd term; set = 1 if no 3rd term

21 PSerr power2 - exponent for 3rd term; set = 0 if no third term

22 TDC - Dewpoint correction factor

23

24 RAC - APN-159 RA correction for cable length

25

*

* Array - NAME

*

* Each entry is a three integer program name used in an EXEC 9 or 10 call

*

Entry Sched.

Loc. AKA by Description

1 SRQName SSERV SRQ servicing program (or setup)

2 StatName IASRV/ASSRV IAU/ADC extended status requestor

3 FastName IASRV Fast program name (1/10 sec)

4 TapeName Slow Tape handler program name (1 sec)

5 MetName Slow Met. processing program name (1 sec)

6 IoutName Met. IAU Output program (1 sec)

7 DacName Met. DAC Output program (1 sec)

8 GrftName Met. Graphics output routine (1 sec)

9 AFltName Met. Asdl Flight Level Data program (1 sec)

10 SFMRName Met. Step Freq. uWave Rad. calc routine (1 sec)

11 LanName Met. Lan BCast Output program (1 sec)

12 Met.

13 Met.

14 Met.

15 Met.

16

17 DiskName TAPEx Pgm to record RAMS data to disk

18 AComName AFLTx,ASDLx Pgm to handle ASDL-VI communications link

19

20 LblName GRFTx Pgm to read Ftrk labels for FTRKx

*

* Array - IAUCH

*

Array

Loc. Description of pointer

1 INE1 channel - 32 bit serial

2 INE2 channel - 32 bit serial

3 GPS channel - ACIA

4 ISEC(95) channel - APN-232 Radar Altimeter - 32 bit serial

5 ISEC(96) channel - Spare

6 ISEC(97) channel - Spare

7 ISEC(98) channel - APN-159 Radar Alt. synchro - 16 bit PIA

8 ISEC(99) channel - APN-159 RA parallel encoder - 16 bit PIA

9 Time Code Generator #1 - 32 bit serial

10 Time Code Generator #2 - 32 bit serial

11 AVAPS input - ACIA

12 BR2G GPS input - ACIA

13 SFMR input - ACIA

14-24 Single status word channels (spot values) stored in ISEC(108-118)

25 Vaisala Cabin Pressure Channel - ACIA

26 ET Printer Status Channel - 8 bit PIA

27-28 User serial ASCII streams - selected words (see IT1(23-24)) are

stored in ISEC(120-128), 9 words max.

29 Not Used

30 Fixed Format #1 output - ACIA to ADTerm card

31 Fixed Format #2 output - ACIA to ADTerm card

32 Fixed Format #3 output - ACIA to ADTerm card

33 Hassablad data output channel - ACIA

34 ET Printer output channel - 8 bit PIA

35 Flight level data to MARS (Radar data sys) output channel - ACIA

36 Flight level data to AVAPS output channel - ACIA

37-40 Not Used

*

* Array - ISFLG

*

Array Set Cleared

Loc. AKA by by Description

1 ADSDataIn ASSRV Fast Slow data arrived flag

2 ADCStatIn ASSRV requestor ADC extended status arrived flag & count

3 IAUDataIn IASRV Fast IAU data arrived flag and word count

4 IAUStatIn IASRV requestor IAU extended status arrived flag & count

5 ADFDataIn AFSRV Fast ADC fast data arrived flag and word count

6 ADFActive AFSRV AFSRV ADC fast data transfer in progress

7 IsecBad ASSRV Fast System Common being updated; >0 all bad,

<0 ISEC array OK, =0 all OK

8 Tape_Fill Fast Next Buffer in Tape_Buf to be filled

9 Tape_Write TAPEx Next Buffer in Tape_Buf to be written out

10 FastDisab HAL Disable Fast Tape Recording when NE 0

11 IauSrq SSERV Setup flag (MS bit) and status from IAU SRQ

12 AdcSrq SSERV Setup flag and status from ADC SRQ

13 MySession IASRV - Session # RAMS software is running in

14 HtSel METPx mBar level of selected standard HT

15 RwndFlg HAL Tape Rwnd/offline primary (bit 0) and/or sec.

(bit 1) tape unit(s)

16 PScalc HAL - Select PQxM's for PS calc

MS nybl for PS1M, 2nd nybl for PS2M, 3rd

nyble for PS3M. For each nybble 1-4

selects PQ1M-PQ4M; 0 - autoselect

17 PQcalc HAL - Select PSxM's for PQ calc

MS nybl for PQ1M, etc. to LS nybl for

PQ4M. For each nybl 1-3 selects

PS1M-PS3M; 0 - autoselect

18 FlowCalc HAL - Select PQxM's for flow angle calc

MS nybl for AP1, 2nd nybl for BP1, 3rd

nybl for AP2/BP2 (nose). For each nybl

1-6 selects PQ1M-DBPM; 0 - auto select

19 PrStat Fast Fast ET printer status - via IAU

20 StartUp Setup Fast System is starting up - ignore some errors

21 Lu8Stat TAPEx DAT Lu 8 Status - See TAPEx code for info

22 Lu9Stat TAPEx DAT Lu 9 Status " " " " "

23 DiskStat DISKx Disk Recording Status:

>0 - Ready to record; value is # of

records already written to disk

=0 - Initial or status unknown, DISKx

needs to run to determine status

<0 - Disk Unavailable, # is FMP error

24-30 Not Used

*

* Array - ISERR

*

Array Set

Loc. AKA by Description

1 ADCSer ASSRV error in ADC slow data pgm or ADC slow burst

2 IAUerr IASRV error in IAU data pgm or IAU data burst

3 ADCFer AFSRV error in ADC fast data pgm or ADC fast burst

4 FPgmer FASTx error in Fast program

5 TapeEr TAPEx error in tape handler program

6 MetErr METPx error in met. program (sched error)

7 DACerr DACxx error in DAC output program

8 PtrErr PRNTx error in Printer output program (printer not ready)

9 AFltErr AFLTx error in ASDL Flight Level Data output (file error)

10 AComErr ACOMx error in ASDL Communication Program

11 SfSErr SFMRx error in Step Freq. calc prgm (file error)

12 GrphErr GRPHx error in data output to graphics box

13 IOutErr IOUTx error in IAU Output routines

14 DiskErr DISKx error in Disk Recording pgm

15 LanErr LANxx error in Lan BCast output program

16 Lu8Err TAPEx error codes & sense key for DAT Lu 8

17 Lu9Err TAPEx " " " " " " Lu 9

18 Lu8Sense TAPEx sense code & addl sense code for Lu 8

19 Lu9Sense TAPEx " " " " " " Lu 9

20 LuErrCnt TAPEx Write error count for Lu 8 (MS byte) &

Lu 9 (LS Byte) - filled on each rewind

*

* Array - ISINFO

*

Array Set

Loc AKA by Description

1-2 Konfig SETUP Default Configuration File extension

3-5 Mission_Num SETUP Mission Number - stored as 6 ASCII char

6-13 Storm_Name SETUP Storm Name - stored as char; blank filled

14-17 Flight_ID SETUP Flight ID - stored as 8 ASCII char; " "

18-19 Unused

*

* Array - IDERR

*

Array Set

Loc AKA by Description

1 HtErr METPx Acft not close to a Standard height

2 SSTErr METPx Problem w/ESST calc (HRD) 1-alt change,2-alt>2000m

3-RD too noisy,4-initial value still being used

3 SfAErr SFMR5x AOC SFMR calc flags - temp range, # of freq, etc

4 SfQErr SFMR4x Quadrant SFMR calc flags

5-20 Unused

*

* Array - T5

*

Loc AKA Cons Used Description

1 GPA 3M GPS Altitude above MSL in meters

2 GLA 3M GPS latitude in degrees

3 GLO 3M GPS longitude in degrees

4 GGY 3M GPS north velocity in m/s

5 GGX 3M GPS east velocity in m/s

6 GVS 3M GPS vertical speed in m/s

7 CPA BR2G GPS Altitude in meters

8 CLA BR2G GPS Latitude

9 CLO BR2G GPS Longitude

10-11 Spare

12 GEP 3M GPS Spherical Error of Position

13 PDOP 3M GPS Position Dilution of Precision

14 APA INE #1 pressure altitude in meters

15 ALA INE #1 latitude in degrees

16 ALO INE #1 longitude in degrees

17 AGY INE #1 north velocity in m/s

18 AGX INE #1 east velocity in m/s

19 AVS INE #1 vertical speed in m/s

20 ADA INE #1 drift angle in degrees

21 AHD INE #1 heading in degrees

22 APC INE #1 pitch in degrees

23 ARL INE #1 roll in degrees

24 BPA INE #2 pressure altitude in meters

25 BLA INE #2 latitude in degrees

26 BLO INE #2 longitude in degrees

27 BGY INE #2 north velocity in m/s

28 BGX INE #2 east velocity in m/s

29 BVS INE #2 vertical speed in m/s

30 BDA INE #2 drift angle in degrees

31 BHD INE #2 heading in degrees

32 BPC INE #2 pitch in degrees

33 BRL INE #2 roll in degrees

34 SPA Selected Nav. pressure altitude in meters

35 SLA Selected Nav. latitude in degrees

36 SLO Selected Nav. longitude in degrees

37 SGY Selected Nav. north velocity in m/s

38 SGX Selected Nav. east velocity in m/s

39 SVS Selected Nav. vertical speed in m/s

40 SDA Selected Nav. drift angle in degrees

41 SHD Selected Nav. heading in degrees

42 SPC Selected Nav. pitch in degrees

43 SRL Selected Nav. roll in degrees

44 TT1 Total Temp #1 in Celsius

45 TT2 Total Temp #2 in Celsius

46 TT3 Spare

47 TA Selected Ambient Temperature in Celcius

48 TW1 Dewpoint #1 Temp in Celsius

49 TW2 Dewpoint #2 Temp (AOC) in Celsius

50 TW3 Dewpoint #3 Temp (EG&G) in Celsius

51 TD Corrected Dewpoint Temp in Celsius

52 ALW J&W Liquid Water in grams/cubic meter

53 KLW King Liquid Water in grams/cubic meter

54 AAV Vertical Acceleration #1 in m/sec/sec

55 BAV Vertical Acceleration #2 in m/sec/sec

56 BT1 AXBT Channel #1 in Celsius

57 BT2 AXBT Channel #2 in Celsius

58 BT3 AXBT Channel #3 in Celsius

59 CWT CO2 radiometer window temperature in Celsius

60 RS Sidelooking (CO2) Radiometer in Celsius

61 RD Downlooking (Sea Surface) Radiometer in Celsius

62 RU Uplooking Radiometer in Celsius

63 PS1M Raw Static Pres from Wing Tip Rsmnt 1281 in mBar

64 PS2M Raw Static Pres from Copilot Rsmnt 1281 in mBar

65 PS3M Spare

66 PS1 Corrected PS from Wing tip Rosemount 1281 in mBar

67 PS2 Corrected PS from Copilot Rosemount 1281 in mBar

68 PS3 Spare

69 PS Selected PS (either PS1 or PS2) for system calc.

70 PQ Selected PQ (PQ1-PQ4) for system calc.

71 PQ1 Corrected PQ from Wing tip Rosemount 1281 in mBar

72 PQ2 Corrected PQ from Copilot Rosemount 1281 in mBar

73 PQ3 Corrected PQ from Copilot Rosemount 1221F in mBar

74 PQ4 Corrected PQ from Nose Rosemount 1221 in mBars

75 PQ1M Raw Dynamic Pres from Wing tip Rsmnt 1281 in mBar

76 PQ2M Raw Dynamic Pres from Copilot Rsmnt 1281 in mBar

77 PQ3M Raw Dynamic Pres from Copilot Rsmnt 1221F in mbars

78 PQ4M Raw Dynamic Pres from Nose Rosemount 1221 in mBars

79 DAPM Raw Dynamic Pressure (Attack) in millibars

80 DBPM Raw Dynamic Pressure (Sideslip) in millibars

81 QC Ram Pressure from Nose Rosemount 1201 in mBars

82 AP1 Attack Pressure #1 (fuselage) in millibars

83 AP2 Attack Pressure #2 (nose) in millibars

84 BP1 Sideslip Pressure #1 (fuselage) in millibars

85 BP2 Sideslip Pressure #2 (nose) in millibars

86 AAM1 Measured Attack Angle #1 in degrees

87 AAM2 Measured Attack Angle #2 in degrees

88 SAM1 Measured Sideslip Angle #1 in degrees

89 SAM2 Measured Sideslip Angle #2 in degrees

90 AAM Selected AAM

91 SAM Selected SAM

92 AA

93 SA

94 RA1 APN-159 Radar Altitude in meters

95 RA2 APN-232 Radar Altitude in meters

96 RA3 GPS Altitude above MSL in meters

97 RA Selected Radar Altitude in meters

98 GA1 Geopotential Alt. from Selected RA in meters

99 GA2 Geopotential Altitude from GPS in meters

100 GA Selected Geopotential Altitude

101 PA Pressure Altitude in meters

102 TSM True Air Speed in m/s

103 AIAS Indicated Air Speed in m/s

104 GS Ground Speed in m/s

105 TK Track in degrees

106 WX East-West Wind component in m/s

107 WY North-South Wind component in m/s

108 WD Wind Direction in degrees

109 WS Wind Speed in m/s

110 DV D-Value in meters

111 SP Surface Pressure in millibars

112 HT Standard Height in meters

113 RH Relative Humidity in percent

114 VA Vertical Acceleration in m/sec/sec

115 VS Vertical Speed in m/s

116 WZ Vertical Winds in m/s

117 FWZ Spare

118 TV Virtual Temperature in Celsius

119 TN Ambient Temperature in Kelvin

120 AMR Mixing Ratio

121 PT Potential Temperature in Kelvin

122 ET Equivalence Potential Temperature in Kelvin

123 DLT Latitude in whole degrees

124 GLT Remainder minutes of Latitude

125 DLG Longitude in whole degrees

126 GLG Remainder minutes of Longitude

127 TS Horizontal True Air Speed in m/s

128 FWS Filtered Horiz. Wind Speed in m/s

129 CBPS Cabin Pressure (from station 5 sensor) in mBar

130 SFWS Surface Wind Speed from Step Freq. Rad. in m/s

131 SFRR Step Freq. Rad. Rain Rate in mm/hr

132 SFDV Step Freq. Rad. Error Flags

133 SFWSM Same, but for user (UMass or Quadrant) SFMR

134 SFRRM

135 SFDVM

136 GDIFC 3M GPS - BR2G GPS position difference in meters

137 GDIF1 3M GPS-INE#1 position difference in meters

138 GDIF2 3M GPS-INE#2 position difference in meters

139 UVH UV Hygrometer

140 LMAPH Lyman Alpha Hygrometer

141 TT4 Total Temp #4 in Celsius

142 TT5 Total Temp #5 in Celsius

143 VDIF1 GPS-INE#1 velocity difference in m/s

144 VDIF2 GPS-INE#2 velocity difference in m/s

145 UPYR1 Up Pyranometer #1 in watts/sq. meter

146 UPYR2 Up Pyranometer #2 "

147 UPYR3 Up Pyranometer #3 "

148 UPYGO Up Pyrgeometer "

149 UDOME Up Pyrgeo dome temp in Celsius

150 UCASE Up Pyrgeo case temp in Celsius

151 DPYR1 Down Pyranometer #1 in watts/sq. meter

152 DPYR2 Down Pyranometer #2 "

153 DPYR3 Down Pyranometer #3 "

154 DPYGO Down Pyrgeometer "

155 DDOME Down Pyrgeo dome temp in Celsius

156 DCASE Down Pyrgeo case temp in Celsius

157 UPYGC Corrected Up Pyrgeometer in watts/sq. meter

158 DPYGC Corrected Down Pyrgeo "

159-162 Spare

163 SFSLPM HRD SFMR Temp Loc for Slope of curve fit

164 SFOFFM HRD SFMR Temp Loc for Offset of curve fit

165-170 SFRL0M-5M HRD SFMR Residuals

171 SFDEVM HRD SFMR Std Deviation

172-177 SFTB0M-5M HRD SFMR Brightness Temperatures in Kelvin

178 SFTNSM " " Noise Source Temp in Kelvin

179 SFTDKM " " Dicke Load Temp in Kelvin

180 SFTWVM " " Waveguide Adapter Temp in Kelvin

181 SFSLP AOC SFMR Temp Loc for Slope of curve fit

182 SFOFF AOC SFMR Temp Loc for Offset of curve fit

183-188 SFRL0-5 AOC SFMR Residuals

189 SFDEV AOC SFMR Std Deviation

190-195 SFTB0-5 AOC SFMR Brightness Temperatures in Kelvin

196 SFTNS " " Noise Source Temp in Kelvin

197 SFTDK " " Dicke Load Temp in Kelvin

198 SFTWV " " Waveguide Adapter Temp in Kelvin

199 SFIPS " " Internal Pressure in PSI

200 DS1PS AVAPS Chan#1 Static Pres in mBar

201 DS1TA " " Ambient Temp in Celsius

202 DS1RH " " Relative Humidity in %

203 DS1WD " " Wind Direction in Deg

204 DS1WS " " Wind Speed in m/s

205 DS1VS " " Sonde Vertical Vel. in m/s

206 DS1LO " " Longitude in Deg

207 DS1LA " " Latitude in Deg

208 DS1GA " " Geopotential Altitude in m

209-217 DS2PS-DS2GA AVAPS Chan#2 data - same sequence as #1

218-226 DS3PS-DS3GA AVAPS Chan#3 data - same sequence as #1

227-235 DS4PS-DS4GA AVAPS Chan#4 data - same sequence as #1

236-250 Spare

*

* Array - ASDLDAT

* These place designations are used by AFLTx to produce averages for

* both MinOb data and for use by the ASDLx program to create RECCO

* messages. All parameters except time are averaged over AsdFltr

* seconds.

*

Loc AKA Description

1 Time_A Time of data - HHMMSS

2 LA_A Latitude - Deg

3 LO_A Longitude - Deg

4 PA_A Pressure Altitude - meters

5 DV_A D-Value - meters

6 TA_A Ambient Temperature - Deg C

7 RD_A Down Radiometer (SST) - Deg C

8 TD_A Dewpoint Temperature - Deg C

9 SP_A Extrapolated Surface Pressure - mBars

10 TV_A Virtual Temperature - Deg C

11 RA_A Radar Altitude - meters

12 GA_A Geopotential Altitude - meters

13 WX_A East-West Wind Speed - m/sec

14 WY_A North-South Wind Speed - m/sec

15-16 Unused

*