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NOAA G-IV
WINTER STORMS 2006
Flight 11 – Track 28
PANC – PANC
Flight ID: 060213N
Sensor or system





Number or Name
Inertial (for wind derivation)  



VEW/VNS


Temperature Probe





AT3
Dew Point Probe





DPLC
Static and Dynamic Pressure




PS2C/QC2C
Project Directory / Constants File



601 / 49cal051
Notes:

There were no time/data glitches during this flight.  Large spikes were seen in the aircraft attitude data at take-off and landing.
AT2 was not installed for these missions.  DPLC was chosen as the primary dewpoint sensor because DPRC was greater than the ambient temperature during ascent and descent.  It also read 5-10 degrees warmer than DPLC through most of the flight.  Because of the ascent data, the data from DPLC appears to be the more accurate of the 2 sensors. 

During ascent and descent, dynamic and differential pressures diverged due to location and air flow around the aircraft.  All data, specifically pressure and wind data should be used carefully during these times.  
DAP1 was operational for this flight; however, since DAP1 has not been working well recently, raw dynamic attack pressure right (DAP2) was still used for derivations.
Turbulence was felt from 2135-2150Z.  This was reflected in the aircraft data.

The _PITR inertial dropped out from 0052Z – 0056Z.  This was reflected in all of the _PITR data.  Wind data should also be ignored during this time period.

All other instruments worked properly.





Takeoff


Landing

Aircraft Static Pressure (mb)

1025.6 mb

1031.5 mb

Station Altimeter


1027.0 mb

30.57”
Flight Director:

Contact Paul Flaherty
Phone #:


(813) 828-3310 ext.  3094






