NOAA P-3 N42RF

SFMR Calibration Flight

Flight ID: 060525H

Sensor or system	Number or Name

INE	2

Accelerometer	2

Temperature Probe	1

Dew Point Probe	2 (Edgetech)

Altitude (for vertical wind)	Radar Altimeter 159

Static Pressure	Rosemount Fuselage

Dynamic Pressure	Rosemount Fuselage 1281

Time Source	Micro 99

Constants File	Not Applicable

Notes:

There were no time/data gaps during this flight.

Radar Altitude data from the 232 sensor was not available from 135705Z through the end of the flight due to calibration needs for the SFMR instrument.

Radar altitude data from the 232 sensor was substituted into the radar altitude 159 data from 132901Z-
135106Z.

There was no altitude data from Inertial 1 and 2 throughout the entire flight.

The King liquid water sensor (KLWC), differential attack pressure from the nose radome (PDAR), differential slip pressure from the nose radome (PDSR), dynamic pressure measured from the center port of the nose radome (PQR), static pressure from the wingtip (PSW), dynamic pressure from the wingtip (PQW), total pressure measured at the nose radome (PTR), total and ambient temperature from sensor 3 (TA3,TT3), and dewpoint sensor 3 (TDM3, TD3), were all inoperative throughout the entire flight.

Takeoff	Landing

Aircraft Static Pressure	1017.6 mb	1017.0 mb

Corrected Tower Pressure	1016.9 mb	1017.6 mb

Flight Director:	Martin Mayeaux (813) 828-3310 ext. 3086