NOAA P-3 N42RF

Ocean Winds Test Flight

Flight ID: 060905H

Sensor or system	Number or Name

INE	1

Accelerometer	1

Temperature Probe	1

Dew Point Probe	1 (General Eastern)

Altitude (for vertical wind)	Radar Altimeter 159

Static Pressure	Rosemount Fuselage

Dynamic Pressure	Rosemount Fuselage 1281

Time Source	Micro 99

Constants File	CO2062.con

Notes:

There were no time/data gaps during this flight.

The King liquid water sensor was inoperative throughout the flight.

Altitude from inertial one and two were both inoperative throughout the entire flight.

Temperature and dewpoint values from sensor number 3 are also erroneous.

Dynamic slip pressure data from the radome was substituted into the dynamic slip pressure values for the fuselage due to erroneous spikes in the fuselage sensor from 172525Z-173155Z.

SPECIAL NOTE!!!	Locations 80, 81 and 82 of record five on the standard tape contain

vertical ground, vertical air and vertical speeds, respectively, computed

using Dave Jorgensen's vertical wind algorithm.

It is recommended that these values be used for vertical wind analysis.

Takeoff	Landing

Aircraft Static Pressure	1015.8 mb	1014.6 mb

Corrected Tower Pressure	1016.9 mb	1015.9 mb

Flight Director:	Martin Mayeaux (813) 828-3310 ext. 3086