N43RF Analog Source & ADC Channel Assignments

TexAQS - Ozone '06

31 July 06 TL

Analog Source	Instrument	ADC Input	KCON	Analog Source	Instrument	ADC Input	KCON
00	J-W Liquid Water	00	251	48	AXBT Channel #1	48	299
01	Total Temperature #1	01	252	49	AXBT Channel #2	49	300
02	Total Temperature #2	02	253	50	AXBT Channel #3	50	301
03	Dewpoint #1 - General Eastern	03	254	51	CSD - WAS Motor Control	51	302
05	Attack Pressure (AP)	04	255	52	CSD - WAS Can Number	52	303
06	Dynamic Attack Pressure (DAP)	05	256	53	CSD - WAS Manifold Pressure	53	304
07	Sideslip Pressure (BP)	06	257	54	CSD - PAN	54	305
08	Dynamic Sideslip Pressure (DBP)	07	258	55	CSD - PAN Cal	55	306
15	PS1 - Wingtip Rosemount 1281	08	259	56	CSD - N2O5	56	307
04	PQ1 - Wingtip Rosemount 1281	09	260	57	CSD - Dry Extinction (Mm-1)	57	308
10	Down PRT-5 Radiometer (SST)	10	261	58	309
11	262	59	310
09	Side PRT-5 Radiometer (CO2)	12	263	60	311
13	264	61	312
12	Vertical Accelerometer #2	14	265	62	313
11	Vertical Accelerometer #1	15	266	63	314
16	Radome Attack Pressure	16	267	64	315
17	Radome Sideslip Pressure	17	268	65	316
18	PQ4 - Radome Diff Pressure	18	269	66	317
19	Radome Impact Pressure	19	270	67	318
20	Total Temp #3 (Port)	20	271	68	319
21	272	69	320
22	273	70	321
23	274	71	322
24	Dewpoint #2 - EdgeTech Vigilant	24	275	72	323
25	276	73	324
26	277	74	325
27	Dewpoint #3 - TDL	27	278	75	326
28	279	76	327
29	280	77	328
30	WVSS-II	30	281	78	329
31	King Liquid Water	31	282	79	330
32	PS2 - CoPilot Rosemount 1281	32	283	00	A

n

a

l

o

g

O

u

t
33	PQ2 - CoPilot Rosemount 1281	33	284	01
34	PQ3 - CoPilot Rosemount 1221F	34	285	02
35	TT1 Heater Current	35	286	03
36	TT2 Heater Current	36	287	04
37	288	05
38	289	06
39	290	07
40	291	08
41	292	09
42	293	10
43	294	11
44	295	12
45	296	13
46	297	14	TA to TDL 0-10 VDC	14
47	298	15	PS to TDL 0-10VDC	15
DAC	DAF