1

N43RF ERROR SUMMARY

AAMPS CHECKOUT FLIGHT

Flight ID: 20111025I1

Sensor or system	Number or Name

INE	(for wind derivation)	INE1

Accelerometer	AccZfilterI-GPS.1

Temperature Probe	TTM.1

Dew Point Probe	TDM.2 (EgdeTech)

Altitude (for vertical wind)	AltI-GPS.1 (RINU GPS)

Static Pressure	PSF.1

Dynamic Pressure	PQF.2

Constants File	adc/n43_hur11v5.adc

Project Directory /acdata/2011/MET/20111025I1

Notes:

There were no data gaps.

Dewpoint sensor #2 (TDM.2...EdgeTech) erroneous values were replaced with dewpoint sensor #1 (TDM.1...Buck) values during the time frame

165255Z – 165309Z.

Dewpoint sensor #2 (TDM.2...EdgeTech) erroneous values were removed and replaced with dewpoint sensor #3 (TDM.3...Buck) values during the time frame

172040Z – 172126Z using the following equation

TDM.2 = TDM.3 + 2.0

All other instruments worked optimally during the flight.

SPECIAL NOTE!!! The variable names asz_dpj, gsz_dpj and wsz_dpj in the netCDF file represent vertical air speeds, vertical ground speeds and vertical wind speeds, respectively, computed using Dave Jorgensen’s vertical wind algorithm. It is recommended that these values be used for vertical wind analysis.

Takeoff (1645Z) Landing (1735Z)

Aircraft Static Pressure 1021.2mb	1020.2mb

Corrected Tower Pressure 1020.2mb	1019.5mb

Flight Director: A. Barry Damiano (813) 828-3310 ext. 3073

2005-10-14T11:04:00