Cal Update	Description	Manufacturer	Model	Serial Number	C0

Slope	C1

Offset
Flow Angle (DAP)	Rosemount	1221F2AF7B1B	842	17.2537	- 0.1021
Flow Angle (DBP)	Rosemount	1221F2AF7B1B	861	17.1471	0.1028
Flow Angle (AP)	Rosemount	1221F2VL7B1B	877	6.8881	0.0641
Flow Angle (BP)	Rosemount	1221F2VL7B1B	878	6.8910	- 0.0437
Copilot (PQ3/PQF2)	Rosemount	1221F2AF7B1B	2443	17.2312	0.8782
Copilot (PQ2/PQF1)	Rosemount	1281B2BEP3	161	16.5540	- 0.3379
Copilot (PS2/PSF)	Rosemount	1281B2BEP3	161	79.9650	249.2979
Wingtip (PQ)	Rosemount	1281B2BEP3	163	16.7537	- 10.2298
Wingtip (PS)	Rosemount	1281B2BEP3	163	79.9704	249.4970
Cabin Pressure	Vaisala	PTB 220	W3120001	120.000	500.000
Radome Flow Angle (Attack)	Rosemount	1221F2 VL7B1B	2317	6.8765	- 0.3298
Radome Flow Angle (Sideslip)	Rosemount	1221F1VL1B1B	879	6.8833	- 0.0814
Radome Flow Angle (Dynamic)	Rosemount	1221F1AF1B1B	286	34.5926	- 0.7240
Radome Flow Angle (Total)	Rosemount	1201F2A14A1A	260	206.8766	- 2.5857
Total Temp 1 (TT1)

(Fwd)	Rosemount	102CH2AF

w/ 510DY1	58171

w/ amp #16	12.0289	- 0.1002
Total Temp 2 (TT2)

(Aft)	Rosemount	102CP2AF

w/ 510GB41E	A7775

w/ amp #152	6.9934	0.0565
Total Temp 3 (TT3)

(Radome)	Rosemount	102CL2AZ

w/ 510GB43E	N/A

Cal Update	Description	Manufacturer	Model	Serial Number	C3

(X3)	C2

(X2)	C1

(X)	C0
CO2 Radiometer	Barnes	PRT-5	N/A
SST Down Radiometer	Barnes	PRT-5	588	0.0906	-0.3626	8.1467	5.4626
SST Up

Radiometer	Barnes	PRT-5	N/A
Dewpoint #1	General Eastern	1201 w/ 1011B	52724 w/

52722	11.1886	- 16.8561
Dewpoint #2	EdgeTech	Vigilant w/

137	29833 w/ 1744	20.0	-60.0
Dewpoint/

Water Vapor	MayComm	TDL	1	7.5	-25.0
Water Vapor	SpectraSensors	WVSS II	1	8000.0	0