N49RF CHANNEL ASSIGNMENT SHEET AND CALIBRATION COEFFICIENTS

Update: 29 July 2003 Original Calibration: 9 June 2003

DSM	CHA N	UPDATE

Updated

DESCRIPTION	MANUF.	MODEL	SERIAL NUMBER	RANGE (V)

C1	C2	C3	C4
FWD	00	Left AOA AP (AP1)	Rosemount	1221F2VL7B1B	2299	+/- 10	0.0248	6.8836
FWD	01	Left AOA DAPM (DAP1)	Rosemount	1221F2AF8B1B	2312	0 - 10	0.9098	34.4696
FWD	02	Right AOA AP (AP2)	Rosemount	1221F2VL7B1B	2309	+/- 10	- 0.0069	6.8884
FWD	03	Right AOA DAPM (DAP2)	Rosemount	1221F2AF8B1B	2313	0 - 10	-0.6441	34.4752
FWD	04	Top Slip BP (BP1)	Rosemount	1221F2VL7B1B	2300	+/- 10	-0.0258	6.8954
FWD	05	Top Slip DBPM (DBP1)	Rosemount	1221F2AF8B1B	2319	0 - 10	-0.3069	34.4634
FWD	06	Bottom Slip BP (BP2)	Rosemount	1221F2VL7B1B	2310	+/- 10	0.0254	6.8888
FWD	07	Bottom Slip DBPM (DBPM2)	Rosemount	1221F2AF8B1B	2318	0 - 10	-1.1433	34.4807
FWD	08	Left Dewpoint (DPL)	EdgeTech	137-C3 Ext. Range	1685 / 018269	0 - 5	-100.0684	30.0875
FWD	09	Right Dewpoint (DPR)	EdgeTech	137-C3 Ext. Range	1686 / 018268	0 - 5	-100.0279	30.0744
FWD	0a	Total Temp #3 (TT3)	Rosemount	102LJ2AG w/ 510GB41E	A32555/0202	+/- 10	-0.1642	7.0160
FWD	0b	07/29/03	Total Temp #2 (TT2)	Rosemount	102CL2AZ w/ 510GB43E	A311920/0199	+/- 10	-0.0030	6.9800
FWD	0c	Total Temp #4 (TT4)	Rosemount	102CP2AF w/ 510GB41E	A6786 /0141	+/- 10	-0.0110	7.0073
FWD	0d	Total Temp #1 (TT1)	Rosemount	102CP2AF w/ 510GB41E	A6784 / 0140	+/- 10	0.3295	7.0075
FWD	0e	07/29/03	Static Pressure #1 (PS1M)	Rosemount	1281AF2B1B	588	0 - 10	-0.2887	108.3443
FWD	0f	Dynamic Pressure #1 (QC1M)	Rosemount	1281AF2B1B	588	0 - 10	0.4596	33.8803
FWD	10	07/29/03	Static Pressure #2 (PS2M)	Rosemount	1281AF2B1B	587	0 - 10	-1.9915	108.4285
FWD	11	Dynamic Pressure #2 (QC2M)	Rosemount	1281AF2B1B	587	0 - 10	0.4244	33.8682
FWD	12	Cryo Hygrometer	Buck	CR-2	207	0 - 10	0	100.0000
FWD	13	Cryo Hygrometer Pressure	Buck	CR-2	207	0-10	0.0000	100.0000
FWD	14	Cabin Pressure	Vaisala	PTB220	W312002	0-5	499.0000	120.0000

RJM/JCPB

for D(Eng. Units) = C1 + C2 * Volts.	C1new= C2new * offset(ADC offset(0,10)) + C1.	C2new= C2 / G(ADC gain(1,2,4,20)).