1

NOAA G-IV ERROR SUMMARY

WINTER STORMS 2007

FERRY FROM MacDILL TO HONOLULU

Flight ID: N070116

Sensor or system	Number or Name

INE	(for wind derivation)	VEW_PITR, VNS_PITR

Accelerometer	ACINS_PITR

Temperature Probe	AT3

Dew Point Probe	DPRC

Static Pressure	PS2M

Dynamic Pressure	QC2M

Attack Angle	AKRD1

Slip Angle	SSRD1

Vert. Wind	PALT

Constants File 49cal061

Project Directory	/proj/701

Local surface observation not current or unavailable.

Notes:

A refueling stop was made in Mesa, AZ with a duration of 70 minutes.

There were no data gaps.

The Total Temperature #2 (TT2) probe was not available for this mission.

All other instruments worked optimally during the flight.

Takeoff	Landing

Aircraft Static Pressure 1022.2mb/973.8mb	973.8mb/1016.9mb

Corrected Tower Pressure 1022.0mb/973.5mb	973.5mb/1017.3mb

Flight Director:	A. Barry Damiano (813) 828-3310 ext. 3073

A. Barry Damiano

2005-06-21T10:07:00