NOAA G-IV N49RF

Winter Storms 2007 Track 56

Flight ID: N070225

Sensor or system	Number or Name

INE (for wind derivation)	VEW_PITR,VNS_PITR

Attack Angle	AKRD2

Slip Angle	SSRD2

Accelerometer	ACINS_PITR

Temperature Probe	AT1

Dew Point Probe	DPRC

Altitude (for vertical wind derivation)	RA

Static Pressure	PS2C

Dynamic Pressure	QC2C

True Air Speed	TAS1

Constants File	49cal062

Project Directory	701

Local Met Data:

PHNL 1853Z 05006KT P6SM SCT040 SCT050 24/18 A3005

PHNL 0153Z 06012KT P6SM FEW034 27/17 A2997

Notes:

There were no time/data gaps during this flight.

Total Temperature number 2 along with air temperature number 2 were not installed and therefore inoperative throughout the flight.

The left dewpoint sensor was ~7 degrees too warm throughout the flight and became inoperative for around 9 minutes from approximately 025300Z through the end of the flight.

The date listed in the header file is also erroneous. However, it has no impact on the flight level data.

Flight Director:	Marty Mayeaux (813) 828-3310 ext. 3086