NOAA G-IV N49RF

Winter Storms 2007 Track 34

Flight ID: N070307N

Sensor or system	Number or Name

INE (for wind derivation)	VEW,VNS

Attack Angle	AKRD2

Slip Angle	SSRD2

Accelerometer	ACINS

Temperature Probe	AT3

Dew Point Probe	DPRC

Altitude (for vertical wind derivation)	RA

Static Pressure	PS2C

Dynamic Pressure	QC2C

True Air Speed	TAS1

Constants File	49cal062

Project Directory	701

Local Met Data:

PHNL 1853Z 00000KT P6SM FEW028 24/18 A3005

PHNL 0053Z 16007KT P6SM FEW050 27/17 A2996

Notes:

There were no time/data gaps during this flight.

Total Temperature number 2 along with air temperature number 2 were not installed and therefore inoperative throughout the flight.

The left dewpoint sensor was ~7 degrees too warm throughout the flight.

Total temperature and ambient temperature from sensor number one showed minor erroneous oscillations throughout the flight.

The flight date listed in the header file is also erroneous. However, it has no impact on the flight level data.

The left dewpoint sensor was inoperative from 021446Z through the end of the flight.

Flight Director:	Marty Mayeaux (813) 828-3310 ext. 3086