1

NOAA G-IV ERROR SUMMARY

HURRICANE 2007

Dist. in Gulf of Mexico

Flight ID: N070919

Sensor or system	Number or Name

INE	(for wind derivation)	VEW_PITR, VNS_PITR

Accelerometer	ACINS_PITR

Temperature Probe	AT3

Dew Point Probe	DPRC

Static Pressure	PS2M

Dynamic Pressure	QC2M

Attack Angle	AKRD1

Slip Angle	SSRD2

Vert. Wind	PALT

Constants File 49cal071

Project Directory	/proj/706

Local surface observation not current or unavailable.

Takeoff at 1720Z Land at 0118Z

Notes:

There were no data gaps.

The Total Temperature #2 (TT2) probe was not available for this mission.

Dynamic slip pressure #1...DBP1...exhibited erroneous data from 2040Z - 0101Z.

This did not impact any meteorological derivations since it was not selected.

All other instruments worked optimally during the flight.

All 32 tempdrop messages were successfully sent to NHC and made it into the 20/00Z model run.

Takeoff	Landing

Aircraft Static Pressure 1012.6mb 1009.6mb

Corrected Tower Pressure 1012.4mb	1010.0mb

Flight Director:	A. Barry Damiano (813) 828-3310 ext. 3073

A. Barry Damiano

2005-06-21T10:07:00