1

N42RF ERROR SUMMARY

P-3/G-4 FORMATION TRAINER

Flight ID: 20121116H1

Sensor or system	Number or Name

INE	(for wind derivation)	INE1

Accelerometer	AccZfilterI-GPS.1

Temperature Probe	TTM.1

Dew Point Probe	TDM.2 (EdgeTech)

Altitude (for vertical wind)	AltI-GPS.1 (RINU GPS)

Static Pressure	PSM.2

Dynamic Pressure	PQM.2

Constants File	adc/n42_hur11v5.adc

Project Directory /acdata/2012/MET/20121116H1

Notes:

There was no flight director onboard.

There were no data gaps.

Dewpoint sensor #2 (TDM2...EdgeTech) had erroneous values during the following time frames: 132702Z – 132732Z and135942Z – 140010Z. The erroneous data was removed and replaced with data from TDM.1 via direct substitution.... TDM.2 = TDM.1.

SPECIAL NOTE!!! The variable names DPJ_GSZ, DPJ_ASZ and DPJ_WSZ in the netCDF file represent vertical ground speed, vertical air speed and vertical wind speed, respectively, computed using Dave Jorgensen’s vertical wind algorithm. It is recommended that these values be used for vertical wind analysis.

There were special surface obs taken by KMCF at 1231Z.

Takeoff (1238Z)

Corrected Tower Pressure 1020.73mb

accounts for station elev. and sensor location

PSM.1	1019.05mb (spot value)

1019.02mb (avg. over 123645Z – 123712Z)

PSM.18 (A->D) 1019.70mb (spot value)

1019.70mb (avg. over 123645Z – 123712Z)

PSM.2 1021.42mb (spot value)

1021.14mb (avg. over 123645Z – 123712Z)

PSM.19 (A->D) 1019.76mb (spot value)

1019.55mb (avg. over 123645Z - 123712Z)

average turning on to active runway

There were special surface obs taken by KMCF at 1528Z.

Landing (1525Z)

Corrected Tower Pressure 1021.75mb

accounts for station elev. and sensor location

PSM.1 1020.40mb (spot value)

1020.30mb (avg. over 152525Z – 152635Z)

PSM.18 (A->D) 1020.39mb (spot value)

1022.30mb (avg. over 152525Z – 152635Z)

PSM.2 1022.96mb (spot value)

1023.05mb (avg. over 152525Z – 152635Z)

PSM.19 (A->D) 1021.95mb (spot value)

1021.92mb(avg. over 152525Z - 152635Z)

average turning off active runway

Flight Director: A. Barry Damiano (813) 828-3310 ext. 3073

2005-10-14T11:04:00